R651.  Natural Resources, Parks and Recreation.
R651-218.  Carburetor Backfire Flame Control.
R651-218-1.  Acceptable Means Of Backfire Flame Control.
	(1)  The following are acceptable means of backfire flame control:
	(a)  an approved flame arrestor secured to the air intake with flametight connection;
	(b)  an approved engine air and fuel induction system; or
	(c)  an attachment to the carburetor or location of the engine air induction system where a flame caused by engine backfire will be dispersed outside the vessel in a manner that the flame will not endanger the vessel or passengers.  All attachments shall be of metallic construction with flametight connections and secured to withstand vibration, shock, and engine backfire.

KEY:  boating
Date of Enactment or Last Substantive Amendment:  1987
Notice of Continuation:  January 7, 2016
Authorizing, and Implemented or Interpreted Law:  73-18-8(5)